**Профессиональные тона COSM и i-CUBE LINK**

**Rated Power Output**

20 W

**Nominal Input Level (1 kHz)**

INPUT: -10 dBu  
i-CUBE LINK/AUX IN: -10 dBu

**Input Impedance**

INPUT: 1 M ohm

**Speaker**

20 cm (8 tommer) x 1

**Controls**

POWER switch  
JC CLEAN button  
LEAD button  
SOLO (MEMORY) button  
TUNER button  
BASS knob  
MIDDLE knob  
TREBLE knob  
EFX knob (CHORUS, FLANGER, PHASER, TREMOLO, HEAVY OCTAVE)  
DELAY knob (WARM, CLEAR)  
REVERB knob (SPRING, PLATE)  
MASTER knob  
[JC CLEAN Channel]  
VOLUME knob  
[LEAD Channel]  
TYPE switch (ACOUSTIC SIM, OVERDRIVE, DISTORTION, METAL, METAL STACK, EXTREME)  
GAIN knob  
VOLUME knob

**Indicators**

JC CLEAN  
LEAD  
SOLO (MEMORY)  
EFX  
DELAY  
REVERB  
TUNER

**Connectors**

INPUT jack: 1/4-inch phone type  
i-CUBE LINK/AUX IN jack: 4-pole miniature phone type  
RECORDING OUT/PHONES jack: Stereo 1/4-inch phone type  
FOOT SW (TIP: JC CLEAN/LEAD, RING: SOLO) jack: 1/4-inch TRS phone type  
AC IN jack

**Power Consumption**

24 W

**Accessories**

Owner's manual  
Power cord  
Mini cable (4-pole miniature phone type)

**Options (sold separately)**

Footswitch (BOSS FS-5U, BOSS FS-6)

**Stoerrelse Og Vaet**

**Width**

378 mm  
14-15/16 tommer

**Depth**

221 mm  
8-3/4 tommer

**Height**

384 mm  
15-1/8 tommer

**Weight**

7.6 kg  
16 lbs. 13 oz.

* 20 ваттный усилитель с специально изготовленными динамиками 8 дюймов
* Три канала: JC CLEAN, LEAD (шесть типов), и SOLO
* Канал SOLO полностью программируемый, позволяющий вам сохранять и запоминать оба канала, чистый и лид, настройки эффектов и эквалайзера
* Три независимых секции эффектов: шесть типов эффектов, дилей и ревер
* Легкое переключение каналов с помощью дополнительный футсвитчей
* i-CUBE LINK позволяет работать с вашим iPhone, iPad или iPod
* Бесплатное приложение CUBE JAM для ваших iOS приборов для воспроизведения треков, джема и записи
* Трехполосный эквалайзер и встроенный тюнер
* Вход RECORDING OUT/PHONES для тихой игры или записи