**Профессиональные тона COSM и i-CUBE LINK**

**Rated Power Output**

20 W

**Nominal Input Level (1 kHz)**

INPUT: -10 dBu
i-CUBE LINK/AUX IN: -10 dBu

**Input Impedance**

INPUT: 1 M ohm

**Speaker**

20 cm (8 tommer) x 1

**Controls**

POWER switch
JC CLEAN button
LEAD button
SOLO (MEMORY) button
TUNER button
BASS knob
MIDDLE knob
TREBLE knob
EFX knob (CHORUS, FLANGER, PHASER, TREMOLO, HEAVY OCTAVE)
DELAY knob (WARM, CLEAR)
REVERB knob (SPRING, PLATE)
MASTER knob
[JC CLEAN Channel]
VOLUME knob
[LEAD Channel]
TYPE switch (ACOUSTIC SIM, OVERDRIVE, DISTORTION, METAL, METAL STACK, EXTREME)
GAIN knob
VOLUME knob

**Indicators**

JC CLEAN
LEAD
SOLO (MEMORY)
EFX
DELAY
REVERB
TUNER

**Connectors**

INPUT jack: 1/4-inch phone type
i-CUBE LINK/AUX IN jack: 4-pole miniature phone type
RECORDING OUT/PHONES jack: Stereo 1/4-inch phone type
FOOT SW (TIP: JC CLEAN/LEAD, RING: SOLO) jack: 1/4-inch TRS phone type
AC IN jack

**Power Consumption**

24 W

**Accessories**

Owner's manual
Power cord
Mini cable (4-pole miniature phone type)

**Options (sold separately)**

Footswitch (BOSS FS-5U, BOSS FS-6)

**Stoerrelse Og Vaet**

**Width**

378 mm
14-15/16 tommer

**Depth**

221 mm
8-3/4 tommer

**Height**

384 mm
15-1/8 tommer

**Weight**

7.6 kg
16 lbs. 13 oz.

* 20 ваттный усилитель с специально изготовленными динамиками 8 дюймов
* Три канала: JC CLEAN, LEAD (шесть типов), и SOLO
* Канал SOLO полностью программируемый, позволяющий вам сохранять и запоминать оба канала, чистый и лид, настройки эффектов и эквалайзера
* Три независимых секции эффектов: шесть типов эффектов, дилей и ревер
* Легкое переключение каналов с помощью дополнительный футсвитчей
* i-CUBE LINK позволяет работать с вашим iPhone, iPad или iPod
* Бесплатное приложение CUBE JAM для ваших iOS приборов для воспроизведения треков, джема и записи
* Трехполосный эквалайзер и встроенный тюнер
* Вход RECORDING OUT/PHONES для тихой игры или записи